<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="2" y1="20" x2="38" y2="20" width="0" layer="20"/>
<wire x1="38" y1="20" x2="40" y2="18" width="0" layer="20" curve="-90"/>
<wire x1="40" y1="18" x2="40" y2="17" width="0" layer="20"/>
<wire x1="2" y1="20" x2="0" y2="18" width="0" layer="20" curve="90"/>
<wire x1="0" y1="18" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="40" y1="3" x2="40" y2="2" width="0" layer="20"/>
<wire x1="40" y1="2" x2="38" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="38" y1="0" x2="2" y2="0" width="0" layer="20"/>
<circle x="5" y="18" radius="1.143" width="0.0254" layer="20"/>
<circle x="5" y="2" radius="1.143" width="0.0254" layer="20"/>
<wire x1="34" y1="17" x2="34" y2="3" width="0" layer="20"/>
<wire x1="34" y1="17" x2="40" y2="17" width="0" layer="20"/>
<wire x1="34" y1="3" x2="40" y2="3" width="0" layer="20"/>
<text>Crowtail- </text>
<text>BLE Module</text>
<text>v0.9</text>
<text>www.elecrow.com</text>
<text>U</text>
<text>GND</text>
<text>VCC</text>
<text>RX</text>
<text>TX</text>
</plain>
<libraries>
<library name="template">
<packages>
<package name="16P-18.5X13.5X0.8">
</package>
</packages>
</library>
<library name="Discrete">
<packages>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="R0603">
</package>
<package name="LED-0603">
</package>
<package name="AVX-B">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ICs_v54">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="CPT_SMD">
<packages>
<package name="0805_S">
</package>
<package name="0603_S">
</package>
</packages>
</library>
<library name="Connector">
<packages>
<package name="4P-SMD-2.0-90D">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="template" package="16P-18.5X13.5X0.8" value="HM-11">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Discrete" package="C0603" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R5" library="Discrete" package="R0603" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Discrete" package="LED-0603" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Discrete" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Discrete" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="Discrete" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Discrete" package="R0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="Discrete" package="AVX-B" value="47uF/10v">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q3" library="Discrete" package="SOT23" value="BSN20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q4" library="Discrete" package="SOT23" value="BSN20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="ICs_v54" package="SOT23-5" value="MIC5205_3.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="CPT_SMD" package="0805_S" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="CPT_SMD" package="0805_S" value="10uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="CPT_SMD" package="0603_S" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Connector" package="4P-SMD-2.0-90D" value="">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="U1" pad="12"/>
<contactref element="D1" pad="-"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="SS2"/>
<contactref element="J1" pad="SS1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="LED">
<contactref element="U1" pad="15"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="+"/>
</signal>
<signal name="BT_RX">
<contactref element="R2" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="BT_TX">
<contactref element="R4" pad="1"/>
<contactref element="Q4" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VCC_3V3">
<contactref element="R1" pad="1"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="Q4" pad="1"/>
<contactref element="U1" pad="9"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="+"/>
<contactref element="U2" pad="5"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="R3" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="R1" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="4"/>
<contactref element="C3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
